jer - ROSAT rgb Images : R_RGB/JER t.ps (r_rgb/jer), 2000-05-20/18:07:58, P 1

ROSAT PSPCB POINTING UK800622P

Field Title: Cygnus-A

0 20 40 50 100 150 200 250 300

z value (cts/s/deg**2)

PI channel

PI channels events energy range z cuts (cts/s/deg**2) min(z) max(z) 11 - 39 30386

0.11 - 0.40 keV

0.00 - 10.00

0.15 98.44 40 - 99 34265

0.40 - 1.00 keV

0.00 - 6.00

0.20 451.15 100 - 299 28000

1.00 - 2.40 keV

0.00 - 4.00

0.13 520.18

−30′ 0° +30′

−30′

0°

+30′ 20h 20h 02m

20h 04m 19h 58m 19h 56m

+41° 30′

+41°

+40° 30′

+40°

7

46 63 66 69 71 81 82

83

Projection center:

Field of view:

Image filter:

Observing period: Exposure: Events: Contours: Objects: PI:

equ.: (RA,Dec) = (19h 59m 02s.04, 40° 45′ 00.0″) gal.: (l_II,b_II) = ( 76.1620°, 5.8336°) 1.87° × 1.87° / 448 × 448 pixel equatorial grid, 15.0" / pixel advanced Poisson likelihood (adaptive) + Gauss likelihood threshold 12.0; maximum blocking exponent 3; 1993-Oct-10, 17:00:10 ... 1993-Oct-11, 03:49:27 9293 s ... 0 s (threshold: 465 s) (detector ontime 9442 s) 92651 (totals: 95226 accepted, 10710 rejected) 10.0 100.0 1000.0 10000.0 2RXP: 83; RRA sequence flags: ....F..X FABIAN, Professor, ANDREW,C

ROSAT PSPCB POINTING 9.3 ks

UK800622P Cygnus-A

MPE / 2000-May-20 filtered X-ray color image 0.11 - 2.40 keV

Declination (J2000)

Right Ascension (J2000)

R_RGB /2000-05-20 © jer@mpe.mpg.de http://www.xray.mpe.mpg.de/cgi-bin/rdb